-- ZyXEL Communications Corporation
-- Private Enterprise MIB definition 
  
-- This file describes the ZyXEL Communications Corporation Enterprise MIB.
-- It contains ZyXEL products OIDs, and common managed objects.

-- ZYXEL-HW-MONITOR-MIB.mib
-- Revision 1.10  2016/02/24 

ZYXEL-HW-MONITOR-MIB DEFINITIONS ::= BEGIN
    IMPORTS
	OBJECT-TYPE
		FROM SNMPv2-SMI			-- RFC2578	
		
	MODULE-IDENTITY
		FROM SNMPv2-SMI

	EnabledStatus
		FROM  P-BRIDGE-MIB
	
	DisplayString                                          
	  FROM SNMPv2-TC

	NOTIFICATION-TYPE
		FROM SNMPv2-SMI

	esMgmt			
		FROM ZYXEL-ES-SMI;

	zyxelHwMonitor MODULE-IDENTITY
		LAST-UPDATED	"201207010000Z"    
		ORGANIZATION "Enterprise Solution ZyXEL"     
		CONTACT-INFO
			""	   
		DESCRIPTION
			"The subtree for hardware monitor"
		::= { esMgmt 26 }

	zyxelHwMonitorStatus 			OBJECT IDENTIFIER ::= { zyxelHwMonitor 1 }		
	zyxelHwMonitorNotifications 	OBJECT IDENTIFIER ::= { zyxelHwMonitor 2 }
	zyxelHwMonitorTrapInfoObject	OBJECT IDENTIFIER ::= { zyxelHwMonitor 3 }	
	zyxelHwMonitorSetup 			OBJECT IDENTIFIER ::= { zyxelHwMonitor 4 }	
--  26.HwMonitor

-- 		fanRpmTable
	
        zyxelHwMonitorFanRpmTable	OBJECT-TYPE
        SYNTAX	SEQUENCE OF ZyxelHwMonitorFanRpmEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The table contains HW monitor fan information."
        ::= { zyxelHwMonitorStatus 1 }
        
		zyxelHwMonitorFanRpmEntry OBJECT-TYPE
        SYNTAX	ZyxelHwMonitorFanRpmEntry
        MAX-ACCESS	not-accessible
        STATUS	current
        DESCRIPTION    	
		"An entry contains HW monitor fan information."
        INDEX          	{ zyHwMonitorFanRpmIndex }
        ::= { zyxelHwMonitorFanRpmTable 1 }

        ZyxelHwMonitorFanRpmEntry ::=
           SEQUENCE {
        	zyHwMonitorFanRpmIndex			INTEGER,
        	zyHwMonitorFanRpmDescription	DisplayString,
        	zyHwMonitorFanRpmCurrentValue	INTEGER,
        	zyHwMonitorFanRpmMaxValue		INTEGER,
        	zyHwMonitorFanRpmMinValue		INTEGER,
        	zyHwMonitorFanRpmLowThreshold	INTEGER,
        	zyHwMonitorFanRpmStatus			DisplayString,
        	zyHwMonitorFanRpmDetect			DisplayString

           }

        zyHwMonitorFanRpmIndex OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "Index of fan."
        ::= { zyxelHwMonitorFanRpmEntry 1 }
        
        zyHwMonitorFanRpmDescription OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
		"Fan Description"
        ::= { zyxelHwMonitorFanRpmEntry 2 }

        zyHwMonitorFanRpmCurrentValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Current speed in Revolutions Per Minute (RPM) on the fan."
        ::= { zyxelHwMonitorFanRpmEntry 3 }

        zyHwMonitorFanRpmMaxValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Maximum speed measured in Revolutions Per Minute (RPM) on the fan."
        ::= { zyxelHwMonitorFanRpmEntry 4 }
        
        zyHwMonitorFanRpmMinValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Minimum speed measured in Revolutions Per Minute (RPM) on the fan."
        ::= { zyxelHwMonitorFanRpmEntry 5 }

        zyHwMonitorFanRpmLowThreshold OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The minimum speed at which a normal fan should work."
        ::= { zyxelHwMonitorFanRpmEntry 6 }

        zyHwMonitorFanRpmStatus OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
		"'Normal' indicates that this fan is functioning above the minimum speed. 
		 'Error' indicates that this fan is functioning below the minimum speed."
        ::= { zyxelHwMonitorFanRpmEntry 7 }

        zyHwMonitorFanRpmDetect OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
		"' ' indicates that no detection. 
		 'SFP' indicates that this fan change due to SFP detection."
        ::= { zyxelHwMonitorFanRpmEntry 8 }


-- 		tempTable

        zyxelHwMonitorTemperatureTable	OBJECT-TYPE
        SYNTAX	SEQUENCE OF ZyxelHwMonitorTemperatureEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The table contains HW monitor temperature information."
        ::= { zyxelHwMonitorStatus 2 }
        
		zyxelHwMonitorTemperatureEntry OBJECT-TYPE
        SYNTAX	ZyxelHwMonitorTemperatureEntry
        MAX-ACCESS	not-accessible
        STATUS	current
        DESCRIPTION    	
		"An entry contains HW temperature information."
        INDEX          	{ zyHwMonitorTemperatureIndex }
        ::= { zyxelHwMonitorTemperatureTable 1 }

        ZyxelHwMonitorTemperatureEntry ::=
           SEQUENCE {
        	zyHwMonitorTemperatureIndex			INTEGER,
        	zyHwMonitorTemperatureDescription	DisplayString,
        	zyHwMonitorTemperatureCurrentValue	INTEGER,
        	zyHwMonitorTemperatureMaxValue		INTEGER,
        	zyHwMonitorTemperatureMinValue		INTEGER,
        	zyHwMonitorTemperatureHighThreshold	INTEGER,
        	zyHwMonitorTemperatureStatus		DisplayString
           }

        zyHwMonitorTemperatureIndex OBJECT-TYPE
        SYNTAX  INTEGER 
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "Index of temperature unit."
        ::= { zyxelHwMonitorTemperatureEntry 1 }
        
        zyHwMonitorTemperatureDescription OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Temperature Description"
        ::= { zyxelHwMonitorTemperatureEntry 2 }
        

        zyHwMonitorTemperatureCurrentValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The current temperature measured at this sensor."
        ::= { zyxelHwMonitorTemperatureEntry 3 }

        zyHwMonitorTemperatureMaxValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The maximum temperature measured at this sensor."
        ::= { zyxelHwMonitorTemperatureEntry 4 }
        
        zyHwMonitorTemperatureMinValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The minimum temperature measured at this sensor."
        ::= { zyxelHwMonitorTemperatureEntry 5 }

        zyHwMonitorTemperatureHighThreshold OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The upper temperature limit at this sensor."
        ::= { zyxelHwMonitorTemperatureEntry 6 }

        zyHwMonitorTemperatureStatus OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "'Normal' indicates temperatures below the threshold and 'Error' for those above."
        ::= { zyxelHwMonitorTemperatureEntry 7 }

-- 		voltageTable

        zyxelHwMonitorVoltageTable	OBJECT-TYPE
        SYNTAX	SEQUENCE OF ZyxelHwMonitorVoltageEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The table contains HW monitor voltage information."
        ::= { zyxelHwMonitorStatus 3 }
        
		zyxelHwMonitorVoltageEntry OBJECT-TYPE
        SYNTAX	ZyxelHwMonitorVoltageEntry
        MAX-ACCESS	not-accessible
        STATUS	current
        DESCRIPTION    	
		"An entry contains HW voltage information."
        INDEX          	{ zyHwMonitorVoltageIndex }
        ::= { zyxelHwMonitorVoltageTable 1 }

        ZyxelHwMonitorVoltageEntry ::=
           SEQUENCE {
        	zyHwMonitorVoltageIndex			INTEGER,
        	zyHwMonitorVoltageDescription	DisplayString,
        	zyHwMonitorVoltageCurrentValue	INTEGER,
        	zyHwMonitorVoltageMaxValue		INTEGER,
        	zyHwMonitorVoltageMinValue		INTEGER,
        	zyHwMonitorVoltageNominalValue	INTEGER,
        	zyHwMonitorVoltageLowThreshold	INTEGER,
        	zyHwMonitorVoltageStatus		DisplayString
           }

        zyHwMonitorVoltageIndex OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "Index of voltage."
        ::= { zyxelHwMonitorVoltageEntry 1 }
        
        zyHwMonitorVoltageDescription OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Voltage Description"
        ::= { zyxelHwMonitorVoltageEntry 2 } 

        zyHwMonitorVoltageCurrentValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The current voltage reading."
        ::= { zyxelHwMonitorVoltageEntry 3 }

        zyHwMonitorVoltageMaxValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The maximum voltage measured at this point."
        ::= { zyxelHwMonitorVoltageEntry 4 }
        
        zyHwMonitorVoltageMinValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The minimum voltage measured at this point."
        ::= { zyxelHwMonitorVoltageEntry 5 }

        zyHwMonitorVoltageNominalValue OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The normal voltage at which the switch work."
        ::= { zyxelHwMonitorVoltageEntry 6 }

        zyHwMonitorVoltageLowThreshold OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The minimum voltage at which the switch should work."
        ::= { zyxelHwMonitorVoltageEntry 7 }

        zyHwMonitorVoltageStatus OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "'Normal' indicates that the voltage is within an acceptable operating 
		 range at this point; otherwise 'Error' is displayed."
        ::= { zyxelHwMonitorVoltageEntry 8 }    
  
  
  -- PowerSourceStatus 
 	zyxelHwMonitorPowerSource OBJECT IDENTIFIER  ::= { zyxelHwMonitorStatus 4 } 
        
    zyHwMonitorPowerSourceMode OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The current power source reading (AC prefer, load-sharing)."
        ::= { zyxelHwMonitorPowerSource 1 }

	zyxelHwMonitorPowerSourceTable	OBJECT-TYPE
        SYNTAX	SEQUENCE OF ZyxelHwMonitorPowerSourceEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The table contains HW monitor power source information."
        ::= { zyxelHwMonitorPowerSource 2 }
                
      
	zyxelHwMonitorPowerSourceEntry OBJECT-TYPE
        SYNTAX	ZyxelHwMonitorPowerSourceEntry
        MAX-ACCESS	not-accessible
        STATUS	current
        DESCRIPTION    	
		"An entry contains HW power source information."
        INDEX          	{ zyHwMonitorPowerSourceIndex }
        ::= { zyxelHwMonitorPowerSourceTable 1 }

        ZyxelHwMonitorPowerSourceEntry ::=
           SEQUENCE {
        	zyHwMonitorPowerSourceIndex			        INTEGER,
        	zyHwMonitorPowerSourceType			        DisplayString, 
        	zyHwMonitorPowerSourceStatus		        DisplayString,
			zyHwMonitorPowerSourceDescription	        DisplayString,
			zyHwMonitorPowerSourcePreviousStatus	    DisplayString
         }

        zyHwMonitorPowerSourceIndex OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "Index of power source."
        ::= { zyxelHwMonitorPowerSourceEntry 1 }

        zyHwMonitorPowerSourceType OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The current power source type (AC/DC)."
        ::= { zyxelHwMonitorPowerSourceEntry 2 } 
         
        zyHwMonitorPowerSourceStatus OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The current power source status  (normal, error, absent, present, active, standby, N/A)."
        ::= { zyxelHwMonitorPowerSourceEntry 3 } 
		
		zyHwMonitorPowerSourceDescription OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
		"Power source Description."
        ::= { zyxelHwMonitorPowerSourceEntry 4 }
		
		zyHwMonitorPowerSourcePreviousStatus OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
		"Power source Previous Status  (normal/error/absent/present)."
        ::= { zyxelHwMonitorPowerSourceEntry 5 }
-- *******************************************************************
-- *
-- * zyxelHwMonitorNotifications
-- *
-- ******************************************************************		
	   zyHwMonitorFanSpeedOutOfRange NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorFanRpmIndex,
				zyHwMonitorFanRpmDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Fan speed is out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 1 }
	   
	   zyHwMonitorTemperatureOutOfRange NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorTemperatureIndex,
				zyHwMonitorTemperatureDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Temperature is out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 2 }
	   
	   zyHwMonitorPowerSupplyVoltageOutOfRange NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorVoltageIndex,
				zyHwMonitorVoltageDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Power supply voltage is out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 3 }
	   
	   zyHwMonitorBackupPowerSupplyInUse NOTIFICATION-TYPE    
	   STATUS  current
       DESCRIPTION
       "Backup power in use is fault."
       ::= { zyxelHwMonitorNotifications 4 }
	   
	   zyHwMonitorDyingGasp NOTIFICATION-TYPE      
	   STATUS  current
       DESCRIPTION
       "Unexpected power down or low power is detected."
       ::= { zyxelHwMonitorNotifications 5 }

	   zyHwMonitorFanAirFlowInconsistency NOTIFICATION-TYPE    
	   STATUS  current
       DESCRIPTION
       "FAN airflows are inconsistent."
       ::= { zyxelHwMonitorNotifications 6 }	
       
       zyHwMonitorFanSpeedOutOfRangeRecovered NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorFanRpmIndex,
				zyHwMonitorFanRpmDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Fan speed is recovered from out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 7 }
	   
	   zyHwMonitorTemperatureOutOfRangeRecovered NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorTemperatureIndex,
				zyHwMonitorTemperatureDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Temperature is recovered from out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 8 }
	   
	   zyHwMonitorPowerSupplyVoltageOutOfRangeRecovered NOTIFICATION-TYPE
       OBJECTS {
				zyHwMonitorVoltageIndex,
				zyHwMonitorVoltageDescription
         }       
	   STATUS  current
       DESCRIPTION
       "Power supply voltage is recovered from out of the normal operation range."
       ::= { zyxelHwMonitorNotifications 9 }
	   
	   zyHwMonitorPowerSourceAbnormal NOTIFICATION-TYPE
		OBJECTS {
				zyHwMonitorPowerSourceIndex,
				zyHwMonitorPowerSourceStatus,
				zyHwMonitorPowerSourceDescription,
				zyHwMonitorTrapPowerSourceErrorType
         }   	   
	   STATUS  current
       DESCRIPTION
       "Power source status is change."
       ::= { zyxelHwMonitorNotifications 10 }
	   
	   zyHwMonitorPowerSourceAbnormalRecovered NOTIFICATION-TYPE 
		OBJECTS {
				zyHwMonitorPowerSourceIndex,
				zyHwMonitorPowerSourceStatus,
				zyHwMonitorPowerSourceDescription		
         }   	   
	   STATUS  current
       DESCRIPTION
       "Power source status change to normal."
       ::= { zyxelHwMonitorNotifications 11 }
	   
	  zyHwMonitorPowerSourceStatusChange NOTIFICATION-TYPE 
		OBJECTS {
				zyHwMonitorPowerSourceIndex,
				zyHwMonitorPowerSourcePreviousStatus,
				zyHwMonitorPowerSourceStatus,
				zyHwMonitorPowerSourceDescription,
				zyHwMonitorTrapPowerSourceErrorType
				
         }   	   
	   STATUS  current
       DESCRIPTION
       "Check power source status change situation."
       ::= { zyxelHwMonitorNotifications 12 } 	   
	   
  	  zyHwMonitorFanSpeedChangeDueToDetection NOTIFICATION-TYPE   
  	   OBJECTS {
				zyHwMonitorFanRpmDetect
         }      
	   STATUS  current
       DESCRIPTION
       "Fan speed change due to detection."
       ::= { zyxelHwMonitorNotifications 13 }
      
-- *******************************************************************
-- *
-- * zyxelHwMonitorTrapInfoObject
-- *
-- *******************************************************************		
		zyHwMonitorTrapPowerSourceErrorType OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
			"There are the error type of power source."  
        ::= { zyxelHwMonitorTrapInfoObject 1 }  

-- *******************************************************************
-- *
-- * zyxelHwMonitorSetup
-- *
-- *******************************************************************		
        zyHwMonitorFanControlSfpDetectionState OBJECT-TYPE  
        SYNTAX  EnabledStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION	
        "Enable/disable the fan control action to perform when the switch SFP module temperature reach warm high limitation"
        ::= { zyxelHwMonitorSetup 1 }
END

