-- ZyXEL Communications Corporation
-- Private Enterprise MIB definition 
  
-- This file describes the ZyXEL Communications Corporation Enterprise MIB.
-- It contains ZyXEL products OIDs, and common managed objects.

-- ZYXEL-DVMRP-MIB.mib
-- Revision 1.4  2013/12/06 

ZYXEL-DVMRP-MIB DEFINITIONS ::= BEGIN

    IMPORTS
	OBJECT-TYPE
		FROM SNMPv2-SMI			-- RFC2578	
		
	MODULE-IDENTITY
		FROM SNMPv2-SMI
	
	EnabledStatus
		FROM  P-BRIDGE-MIB

	zyRouteDomainIpAddress, zyRouteDomainIpMaskBits
		FROM ZYXEL-IP-FORWARD-MIB
		
	esMgmt			
		FROM ZYXEL-ES-SMI;

	zyxelDvmrp MODULE-IDENTITY
		LAST-UPDATED	"201207010000Z"    
		ORGANIZATION "Enterprise Solution ZyXEL"     
		CONTACT-INFO
			""	   
		DESCRIPTION
			"The subtree for Distance Vector Multicast Routing Protocol (DVMRP)"
		::= { esMgmt 23 }
		
	zyxelDvmrpSetup     			OBJECT IDENTIFIER ::= { zyxelDvmrp 1 }		

        zyDvmrpState OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "Enable/Disable DVMRP on the switch."
        ::= { zyxelDvmrpSetup 1 }
        
        zyDvmrpThreshold OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The maximum time to live value. This applies only to multicast traffic this switch sends out."
        ::= { zyxelDvmrpSetup 2 }        
        
		zyxelDvmrpRouteDomainTable OBJECT-TYPE
        SYNTAX	SEQUENCE OF ZyxelDvmrpRouteDomainEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The table contains DVMRP configuration."
        ::= { zyxelDvmrpSetup 3 }
        
		zyxelDvmrpRouteDomainEntry OBJECT-TYPE
        SYNTAX	ZyxelDvmrpRouteDomainEntry
        MAX-ACCESS	not-accessible
        STATUS	current
        DESCRIPTION    	
		"An entry contains DVMRP configuration."
        INDEX          	{ zyRouteDomainIpAddress, zyRouteDomainIpMaskBits }
        ::= { zyxelDvmrpRouteDomainTable 1 }

        ZyxelDvmrpRouteDomainEntry ::=
           SEQUENCE {
        	zyDvmrpRouteDomainState		EnabledStatus
           }
                   
        zyDvmrpRouteDomainState OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "Enable/Disable DVMRP on this IP routing domain."
        ::= { zyxelDvmrpRouteDomainEntry 1 }

END

